**Section 1 – Identification of the product and of the company / undertaking**

**1.1 Product identifier**

Coated abrasives group KK

**CS 329 Y, JF; CS 409 Y; CS 410 X; CS 451 X; CS 570; CS 631 XF, JF; CS 661; CS 910 Y, CS 931 JF; GX 931**

**JF; FS 966; GX 712 JF; GX 931 JF; LS 312 JF; LS 313 JF; QMC/QRC 409; QMC/QRC 910**

**1.2 Use of the products**

Coated abrasives for the grinding / sanding of different kinds of materials

**1.3 Details of the supplier**

**COMPANY:** KLINGSPOR Abrasives, Inc.

**ADDRESS:** PO Box 2367, 2555 Tate Blvd., S.E. Hickory, NC 28603-2367

**Telephone:** 828-322-3030

**Fax:** 828-326-0296

**E-mail:** technical@klingspor.com

**1.4 Emergency telephone number:**

1-828-322-3030

**Section 2 – HAZARDS IDENTIFICATION**

Not applicable; not a hazardous substance or mixture. See also section 8 and 16

**2.2 Label elements**

Not applicable. No labeling is required under GHS including precautionary statements as this is not a hazardous substance or mixture.

See also section 8 and 16

**2.3 Hazards not otherwise classified (HNOC) or not covered by GHS**

Not known.

**Section 3 – Composition / information on ingredients**

The products contain the following ingredients which are classified according to Occupational Safety and Health

Administration regulations (29 CFR 1910.1200 – Hazard Communication) or for which a community occupational exposure limit exists:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Substance | EC-N⁰ | CAS-N⁰ | REACHRegistration N⁰ | Conc. (%) | Classification according to OSHA Regulations |
| Hazard statements | GHS hazardclassifications |
| Cryolite (sodium aluminum fluoride) | 237-410-62119511565 | 13775-53-6 | 01-43 | 1 – 5 | Acute toxin (respiratory)Reproductive toxinAquatic toxin (chronic) | 422 |
| Potassiumfluoroborate | 237-928-2 | 14075-53-7 - |  | 3 – 35 | Respiratory irritant (acute)Eye irritant | 1A2 |
|  |  |  |  |  |  |  |

**Section 4 – First aid measures**

See also section 8 and 16

**4.1 Description of first aid measures**

Inhalation: Not possible, due to the form of the products Eye contact: Not possible, due to the form of the products Skin contact: No harmful effects know

Ingestion: Not likely, due to the form of the products; if necessary contact physician

Notes to physician: Not available.

**4.2 Most important symptoms and effects, both acute and delayed**

Not known.

**4.3 Indication of any immediate medical attention and special treatment needed**

Not relevant. Treat symptomatically.

**Section 5 – Fire Fighting Measures**

**5.1 Extinguishing media**

Extinguishing media: water, foam, sand, powder or CO2 as appropriate for surrounding materials.

**5.2 Special hazards arising from the products**

Toxic fumes may occur. Use respiratory equipment.

**5.3 Advice for fire fighters**

Extinguishing media should be selected according to the surrounding area.

**Section 6 – Accidental release measures**

Not applicable.

**Section 7 – HANDLING AND STORAGE**

Follow instructions of grinding machine manufacturers and the relevant national regulations. In addition, observe the safety recommendations of the manufacturer.

Store abrasives in dry, frost-free conditions avoiding wide variations in temperature. Ensure they are properly protected and supported to prevent damage and distortion.

Coated abrasives should be stored at 18-22˚C, 45-65 % relative humidity.

**Section 8 – Exposure controls / personal protection**

**8.1 Control parameters**

Before grinding it is recommended to perform a risk assessment and to use personal protection equipment accordingly.

*Occupational exposure limit values and/or biological limit values*

Keep exposure to the following components under surveillance. (Observe also the regional official regulations).

**Limit**

**Substance EC-N˚ CAS-N˚ Occupational limit value Peak**

**Source,**

**value**

**Long term Short term**

**limit**

**remark**

**type**

**(country of**

**origin)**

**mg/m3 ml/m3**

**(ppm)**

**mg/m3 ml/m3**

**(ppm)**

OSHA (USA)

Cryolite 237

410-6

13775-

53-6

2.5\* - - - HSC,

(flourides,

inorganic as F)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| OSHA(USA) | Potassiumfluoroborate | 237-928-2 | 14075-53-7 | 2.5\* - - - |  |  |  |  | HSC,(flourides,inorganic as F) |
|  |  |  |  |  |  |  |  |  |  |

Note: Hazardous dust of the workpiece material may be generated during grinding and/or sanding operations. National regulations for dust exposure limit values have to be taken into consideration as part of the job hazard assessment.

**8.2 Exposure controls**

8.2.1 Individual protection measures

8.2.1.1. Respiratory protection: Use respiratory protective equipment

(type depends on specific application and material being ground)

8.2.1.2. Hand protection: Wear protective gloves

(type depends on specific application and material being ground)

8.2.1.3. Eye protection: Wear protective goggles or face shield

(type depends on specific application and material being ground)

8.2.1.4. Hearing protection: Use hearing protection

(type depends on specific application and material being ground)

8.2.1.5. Body protection: Use protective clothing

(type depends on specific application and material being ground)

**Section 9 – Physical and chemical properties**

**9.1 Information on basic physical and chemical properties**

9.1.1 Physical state: solid

9.1.2 Color: according to the type of product

9.1.3 Solubility in water: not measured

**9.2 Other information**

None

**Section 10 – Stability and reactivity**

**10.1 Reactivity**

Coated abrasives are stable when handled or stored correctly.

**10.2 Chemical stability**

No decomposition in normal use.

**10.3 Possibility of hazardous reactions**

No dangerous reaction known.

**10.4 Conditions to avoid**

Coated abrasives are stable when handled or stored correctly.

**10.5 Incompatible materials**

No dangerous reactions known.

**10.6 Hazardous decomposition products**

A temperatures exceeding 482˚F (250˚C), hazardous or toxic decomposition products may be generated.

**Section 11 – Toxicological information**

**11.1 Information on toxicological effects**

No toxicological effects if inhaled or swallowed or with eye or skin contact are known. See also section 8.

**Section 12 – Ecological information**

**12.1 Toxicity**

No effects known.

**12.2 Persistence and degradability**

No biodegradable potentials known.

**12.3 Bioaccumulative potential**

No potentials known.

**12.4 Mobility in soil**

No potentials known.

**12.5 Results of PBT and vPvB assessment**

Not relevant.

**12.6 Other adverse effects**

No effects known.

**Section 13 – Disposal considerations**

**13.1 Waste treatment methods**

13.1.1 Product

Follow national and regional regulations.

13.1.2 Packing

Follow national and regional regulations.

**Section 14 – Transport information**

**International transport:** Not classified as a dangerous good under transport regulations **Land transport, USDOT:** Not classified as a dangerous good under transport regulations **Sea transport, IMDG**: Not classified as a dangerous good under transport regulations

**Air transport, IATA/ICAO:** Not classified as a dangerous good under transport regulations

**Section 15 – Regulatory information**

**15.1 Safety, health, and environmental regulations/legislation specific for the products**

No specific labeling requirements under respective GHS directives.

**15.2 Chemical safety assessment**

Not relevant.

**Section 16 – Other information Changes to previous versions** See sections 1 to 16.

**Literature and data sources**

U.S. Department of Labor, Occupational Safety and Health Administration: 29 CFR 1910.1000 (Hazard

Communication)

Transport regulations according to IATA.

**According to United States Regulation OSHA 29 CFR 1910.1200:**

|  |  |  |  |
| --- | --- | --- | --- |
| Substance | Hazard Statements | GHS Hazard Class | Description |
| Cryolite (sodiumaluminum fluoride | Respiratory toxin (acute)Reproductive toxinAquatic toxin (chronic) | 422 | Inhalation of dusts and mists can be harmful.Suspected reproductive toxicant.Harmful / toxic to aquatic life for prolonged exposure. |
| Potassium fluoroborate | Respiratory irritant (acute) Eye Irritant | 1A2 | Inhalation of dusts and mists can be harmful. Can be irritating to eyes. |

------------------------------------------------------------------------------------------------------------------------------------------------------------ The above information is based on our current standard of knowledge and does not constitute any warranty or conditions of this product. The information does not form part of any contractual agreement. It remains the end user’s responsibility to adhere to existing laws and regulations.

**CAUTION: Intentional misuse of this chemical product, as with any industrial chemical in contact with the body, can be harmful or fatal. This includes such things as deliberately breathing, placing in mouth, swallowing, placing on skin, or any other body contact, or repeated or continuous contact.**

*KLINGSPOR Abrasives makes this information in good faith, but makes no representation as to its comprehensiveness or its accuracy. This document is offered as a guide to a trained person, for appropriate precautionary handling. Persons using the product and receiving the information must exercise independent judgment in determining the appropriateness of the use and the safety information for their particular purpose.*